**Adjustable Power Supply: SE-2500-12**



**Product Specifications:**

1. Input: voltage 220V AC, Current 13 A.
2. Working frequency: 50/60Hz
3. Power: 2500W
4. Output voltage : 0 - 12V DC
5. Output current: 0 - 208 A
6. Natural air-cooled
7. LED power indicator
8. 100% full of aging
9. All use 105 °C electrolytic capacitor
10. Safety Compliance: CCC / FCC / CE
11. Working Temperature: -10 ~ 60 ℃
12. Storage Temperature: -20 ~ 65 ℃
13. Ambient Humidity: 20 ~ 90% RH
14. Product size: 280\*180\*65mm
15. Shell material: metal shell, aluminum base

**Features:**

1. Widely used in LED lights, industrial automation, LED display, communication, etc.
2. Protection: short circuit protection, overload protection, over voltage protection.
3. Low heat, energy saving, super safe, environmentally friendly, long service life.
4. Not waterproof: suitable for indoor use; or add waterproof case for outdoor use.
5. Orders usually ship within 24 hours after payment is received.

**Control:**

1. Support 0-5V (0-10V) analog signal control output voltage (linear rise)
2. Support 0-5V (0-10V) analog signal control output current (5%~100%)
3. Support adjustable resistor to control output voltage
4. Support adjustable resistor to control output current
5. Support ON/OFF remote switch machine
6. Support N+1 function
7. Professional installation of qualified electrician is highly

















