**List of extension for Acetic Anhydride Pilot Plant**

1. 2 Flow sensors (1/2 inches) – (stainless steel 316)
2. 3 Temperature sensors (+100 °C) – (stainless steel 316)
3. 5 electrical valves (1/2 inches) – (stainless steel 316)
4. 2 Pressure sensors + 2 safety valves (1/2 inches) – (stainless steel 316)
5. 1 mixer + axe (stainless steel 316)
6. 4 manual valves stainless steel 316
7. Heater

Price $ ???